

1. Download the upgrade tool and upgrade file ,the download address： http://vorke.mediafire.com/file/966mp87g1m01ssc/HD41\_PRO\_UPDATE.zip，Then decompress，you will get two files: VORKE\_HD41 Pro\_Tool.exe and VORKE HD41 PRO\_V2.3\_20170828.bin.
2. Plug in the HD41 PRO power supply,then use the 3.5mm to RS232 cable（in the accessories）put into the machine's RS232 interface, the other end put into the computer's RS232 interface.









1. Run VORKE\_HD41 Pro\_Tool .exe program, Port select COM1, 19200, and then click the Connect button, then click Status. As shown below, the connection was successful.



1. Click the Upgrade button, click Open, select VORKE HD41 PRO\_V2.3\_20170828.bin file, click OK, and then click the Upgrade button, wait until the program appears Firmware upgrade successfully, that upgrade success.





Note: the computer that is upgraded needs a RS232 interface, if your computer does not have RS232 interface, you can buy a USB to RS232 adapter cable（FIDI-FT232 solution）.

